|  |
| --- |
| TDA5144AT Brushless Motor Driver  **Pinout (pins are labelled on the underside of the PCB): VMO** - Power to motor coils (usually 5-9V depending on required speed) **VCC** - Power to controller chip (usually 5-12V). Can be wired to VMO for single supply operation. **GND** – ground **A, B, C** - motor coil terminals **O** - motor coils common centre terminal (use an ohm-meter to establish the centre point; it is the one with the same resistance to the other 3 terminals) **TACHO** – pulse output which can be used to synchronise other circuitry to motor spin  **Sixty-four Pixels**  web: http://six4pix.com, email: [sixtyfourpixels@gmail.com](mailto:sixtyfourpixels@gmail.com) |
| TDA5144AT Brushless Motor Driver  **Pinout (pins are labelled on the underside of the PCB): VMO** - Power to motor coils (usually 5-9V depending on required speed) **VCC** - Power to controller chip (usually 5-12V). Can be wired to VMO for single supply operation. **GND** – ground **A, B, C** - motor coil terminals **O** - motor coils common centre terminal (use an ohm-meter to establish the centre point; it is the one with the same resistance to the other 3 terminals) **TACHO** – pulse output which can be used to synchronise other circuitry to motor spin  **Sixty-four Pixels**  web: http://six4pix.com, email: [sixtyfourpixels@gmail.com](mailto:sixtyfourpixels@gmail.com) |
| TDA5144AT Brushless Motor Driver  **Pinout (pins are labelled on the underside of the PCB): VMO** - Power to motor coils (usually 5-9V depending on required speed) **VCC** - Power to controller chip (usually 5-12V). Can be wired to VMO for single supply operation. **GND** – ground **A, B, C** - motor coil terminals **O** - motor coils common centre terminal (use an ohm-meter to establish the centre point; it is the one with the same resistance to the other 3 terminals) **TACHO** – pulse output which can be used to synchronise other circuitry to motor spin  **Sixty-four Pixels**  web: http://six4pix.com, email: [sixtyfourpixels@gmail.com](mailto:sixtyfourpixels@gmail.com) |
| TDA5144AT Brushless Motor Driver  **Pinout (pins are labelled on the underside of the PCB): VMO** - Power to motor coils (usually 5-9V depending on required speed) **VCC** - Power to controller chip (usually 5-12V). Can be wired to VMO for single supply operation. **GND** – ground **A, B, C** - motor coil terminals **O** - motor coils common centre terminal (use an ohm-meter to establish the centre point; it is the one with the same resistance to the other 3 terminals) **TACHO** – pulse output which can be used to synchronise other circuitry to motor spin  **Sixty-four Pixels**  web: http://six4pix.com, email: [sixtyfourpixels@gmail.com](mailto:sixtyfourpixels@gmail.com) |